**SECTION 01 57 23 - TEMPORARY STORMWATER POLLUTION CONTROL**

Revise this Section by deleting and inserting text to meet Project-specific requirement

1. **GENERAL**

Retain or delete this article in all Sections of Project Manual.

* + - 1. SUMMARY

Section includes temporary stormwater pollution controls.

* + - 1. PREINSTALLATION MEETINGS

Retain "Preinstallation Conference" Paragraph below if Work of this Section is extensive or complex enough to justify a conference.

Preinstallation Conference: Conduct conference at [Project site] <Insert location>.

Meet with Government, and earthwork subcontractor.

Review requirements of the SWPPP, including permitting process, worker training, and inspection and maintenance requirements.

* + - 1. INFORMATIONAL SUBMITTALS

Stormwater Pollution Prevention Plan (SWPP): Within 10 days of Notification of Award and not less than 5 days prior to preconstruction conference, submit completed SWPPP and copy of signed Notice of Intent, NPDES Form 3510-6.

* + - * 1. Inspection reports.
      1. QUALITY ASSURANCE

Stormwater Pollution Prevention Plan (SWPPP) Coordinator: Experienced individual or firm with a record of successful water pollution control management coordination of projects with similar requirements.

SWPPP Coordinator shall complete and finalize the SWPPP form.

SWPPP Coordinator shall be responsible for inspections and maintaining of all requirements of the SWPPP.

Installers: Trained as indicated in the SWPPP.

1. **PRODUCTS**
   * + 1. TEMPORARY STORMWATER POLLUTION CONTROLS

Provide temporary stormwater pollution controls as required by the SWPPP.

1. **EXECUTION**
   * + 1. INSTALLATION

Comply with best management practices, general requirements, performance requirements, reporting requirements, and requirements included in the SWPPP.

* + - * 1. Locate stormwater pollution controls in accordance with the SWPPP.
        2. Conduct construction as required to comply with the SWPPP and that minimize possible contamination or pollution or other undesirable effects.

Inspect, repair, and maintain SWPPP controls during construction.

Inspect all SWPPP controls not less than every 7 days, and after each occurrence of a storm event, as outlined in the SWPPP.

Remove SWPPP controls at completion of construction and restore and stabilize areas disturbed during construction.

**END OF SECTION**